# tecella_reg_props Struct Reference

`#include <TecellaAmp.h>`

## Data Fields
wchar_t | label [TECELLA_REG_PROPS_LABEL_SIZE]
wchar_t | units [TECELLA_REG_PROPS_UNITS_SIZE]
bool | supported
bool | can_be_disabled
double | v_min
double | v_max
double | v_lsb
unsigned int | v_divisions
double | v_default
double | pct_lsb

## Field Documentation

bool tecella_reg_props::can_be_disabled

Indicates if you can disable this register.

wchar_t tecella_reg_props::label[TECELLA_REG_PROPS_LABEL_SIZE]

Label that should be used for this register in a GUI.

double tecella_reg_props::pct_lsb

Indicates the precision of the double value when represented in percent.

bool tecella_reg_props::supported

Indicates if the register is supported by the device.

wchar_t tecella_reg_props::units[TECELLA_REG_PROPS_UNITS_SIZE]

Units used when represented as a double.

double tecella_reg_props::v_default

Default value upon initialization.

unsigned int tecella_reg_props::v_divisions

The number of valid values in the range [v_min,v_max]

double tecella_reg_props::v_lsb

Indicates the precision of the double value.

double tecella_reg_props::v_max

Maximum value for when calling tecella_chan_set().

double tecella_reg_props::v_min

Minimum value for when calling tecella_chan_set().

The documentation for this struct was generated from the following file:

- TecellaAmp.h