# tecella_system_monitor_result Struct Reference

`#include <TecellaAmp.h>`

## Data Fields
wchar_t | label [TECELLA_SYSTEM_MONITOR_RESULT_LABEL_SIZE]
wchar_t | units [TECELLA_SYSTEM_MONITOR_UNITS_LABEL_SIZE]
int | board_index
int | board_result_index
double | value
double | value_expected
double | value_expected_min
double | value_expected_max

## Field Documentation

int tecella_system_monitor_result::board_index

Indicates which board of the system this result is for.

int tecella_system_monitor_result::board_result_index

Indicates the result index for the specified board. Not all that usefull, but you never know.

wchar_t tecella_system_monitor_result::label[TECELLA_SYSTEM_MONITOR_RESULT_LABEL_SIZE]

Label that should be used for this result in a GUI.

wchar_t tecella_system_monitor_result::units[TECELLA_SYSTEM_MONITOR_UNITS_LABEL_SIZE]

Units used for value and value_expected.

double tecella_system_monitor_result::value

The measured value.

double tecella_system_monitor_result::value_expected

The expected value.

double tecella_system_monitor_result::value_expected_max

The minimum expected value. Any value greater than this should be flagged.

double tecella_system_monitor_result::value_expected_min

The minimum expected value. Any value less than this should be flagged.

The documentation for this struct was generated from the following file:

- TecellaAmp.h